|  |
| --- |
| **~~~~ SPECIFIER NOTES ~~~~~***This specification guidelines, its sections, and text included, is intended to be used in the preparation of Contract Documents. It contains* ***Specifier Notes*** *which shall guide editing by the A/E consultant for the uniqueness of each project during the preparation of the Project Manual. Where* ***[Optional]*** *appears in this document, it indicates requirements which may/may not be relevant to the subject project depending upon the project complexity, scope and unique conditions. For* ***DRAFT*** *specifications prepared during the design process, use Microsoft Word, Track Changes. Set Criteria so that deletion show as strikethrough. Deletions and additions are to be in red text.**Notes unique to this section:*1. *The need for this specification section is the sole responsibility of the A/E and is not included as part of the DES Division 01 Specification Guidelines. A/E should consider inclusion of section 01 1101 as means to identify necessary procedures associated existing Hazardous Materials included in the Project*

***~~~ END OF SPECIFIER NOTES ~~~~*** |

**SECTION 01 1101 – SUMMARY OF HAZARDOUS MATERIALS WORK**

**PART 1 - GENERAL**

**1.01 SUMMARY**

A. This Section includes administrative and procedural requirements for hazardous materials.

**1.02 RELATED DOCUMENTS**

A. Drawings and general provisions of the Contract, including General and Supplementary Conditions and other Division 01 Specification Sections, apply to this Section.

B. Section 01 7419 Construction Waste Management and Disposal

**1.03 OWNER NOTIFICATION**

A. The Owner has surveyed the existing site for hazardous materials and has not discovered any known hazardous materials.

B. Owner is to attain a certified environmental consultant to determine any hazardous materials on project site and provide a “Good Faith “ Survey report of the project area which might be impacted by hazardous materials and dangerous wastes.

**1.04 CONTRACTOR NOTIFICATION**

A. Pursuant to WAC 296.62.054 to 296.62.05425, provide the Owner with a complete list of all hazardous chemicals and other materials intended to be used during execution of the project, including storage locations.

**1.05 ASBESTOS CONTAINING MATERIAL AND LEAD PAINT**

A. The Contractor shall bring to the attention of the Architect any material suspected of being hazardous which is encountered during execution of the Work. The Owner will arrange for tests to determine if the material is hazardous. If the material is found to be hazardous, the Owner will initiate the construction modification procedure for its abatement by the Contractor.

B. Compliance with Regulations: All work shall comply with the applicable requirements of 29 CFR 1926/1910. The disposal of any hazardous materials encountered shall also comply with the requirements of applicable state and municipal safety and health requirements. Where there is a conflict between applicable regulations, the most stringent shall apply.

**PART 2 - PRODUCTS (NOT USED)**

**PART 3 - EXECUTION (NOT USED)**

**END OF SECTION 01 1101 – SUMMARY OF HAZARDOUS MATERIALS WORK**